{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":4,"rows_kept":30,"flags":["formulas_cached_only"]}
["Locomotive Pulling Power Estimator"]
[]
["Scale 1:N",160,"1:N"]
[]
["Locomotive Information"]
["MU Count",1,"units"]
["Lcomotive weight",3,"oz/unit"]
["Tractive Effort ",{"v":0.25,"d":"25%"},"%"]
["Tractive Effort",0.75,"oz/unit"]
["Net Tractive Effort",0.75,"oz"]
[]
["Consist Information"]
["Avg. Car Weight",1,"oz/car"]
["Avg. Rolling Resistance",{"v":0.04,"d":"4%"},"%"]
["Avg. Rolling Resistance",0.04,"oz/car"]
[]
["Zero-grade Capacity",18,"cars"]
[]
["Grade Information"]
["Grade",{"v":0.03,"d":"3%"},"%"]
["Added R/car at Grade",0.03,"oz/car"]
["Net R/car",0.07,"oz/car"]
["Added R/MU at grade",0.09,"oz/unit"]
[]
["Curve Information"]
["Radius",0,"in","(Use 0 for tangent)"]
["RR per Degree",{"v":0.0004,"d":"0.04%"},"%"]
["Degree Curvature",0,"deg"]
[]
["Capacity @ Grade+Curve",9,"cars"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}